**Assembly Troubleshooting Guide**

**Issue: Chair is not level**

**Cause:** Chairs can be wobbly or not level if one or more bolts are fully tightened before all bolts are attached.

**Solution:** Loosen each bolt in the seat box (front legs, back corner-blocks and back apron) to the point where they can be turned with your fingers. Place the chair upright on the floor. Firmly press down evenly until product sits level, but do not lean against the chair back. Carefully turn the chair upside down, and tighten each bolt.

**Issue: Holes are misaligned**

**Cause:** This issue can occur when some bolts are tightened fully before all other bolts are attached.

**Solution:** Make sure each bolt in the seat box (front legs, back corner-blocks and back apron) is loosened until it can be turned with your fingers. This will allow you to realign the holes.

**Remember, loosely attach all bolts. Do not over tighten. Once the product is fully assembled, tighten all bolts.**